%@ALM_NC_IO(MAX:1000)
ID: 000 - BitAddr: A0400 - Content: "IOLink Device Not Detected"
ID: 001 - BitAddr: A0401 - Content: "IOLink Too Much IO"
ID: 002 - BitAddr: A0402 - Content: "IOLink Device Feedback Wrong Data"
ID: 003 - BitAddr: A0403 - Content: "IOLink Device No Response"
ID: 004 - BitAddr: A0404 - Content: "IOLink Device Response Wrong Command"
ID: 005 - BitAddr: A0405 - Content: "IOLink Device Response Wrong Struct"
ID: 006 - BitAddr: A0406 - Content: "Inter Comunication GCode Not Reasonable"
%@WARN_NC_IO(MAX:1000)
ID: 000 - BitAddr: A0450 - Content: "IOLink Device Not Detected"
ID: 001 - BitAddr: A0451 - Content: "IOLink Too Much IO"
ID: 002 - BitAddr: A0452 - Content: "IOLink Device Feedback Wrong Data"
ID: 003 - BitAddr: A0453 - Content: "IOLink Device No Response"
ID: 004 - BitAddr: A0454 - Content: "IOLink Device Response Wrong Command"
ID: 005 - BitAddr: A0455 - Content: "IOLink Device Response Wrong Struct"
%@END