%@ALM_NC_OT(MAX:1000)
ID: 000 - BitAddr: A0300 - Content: "Hard Limit X+"
ID: 001 - BitAddr: A0301 - Content: "Hard Limit X-" 
ID: 002 - BitAddr: A0302 - Content: "Hard Limit Y+" 
ID: 003 - BitAddr: A0303 - Content: "Hard Limit Y-"
ID: 004 - BitAddr: A0304 - Content: "Hard Limit Z+"
ID: 005 - BitAddr: A0305 - Content: "Hard Limit Z-"
ID: 006 - BitAddr: A0306 - Content: "Hard Limit A+"
ID: 007 - BitAddr: A0307 - Content: "Hard Limit A-"
ID: 008 - BitAddr: A0308 - Content: "Hard Limit B+"
ID: 009 - BitAddr: A0309 - Content: "Hard Limit B-"
ID: 010 - BitAddr: A0310 - Content: "Hard Limit C+"
ID: 011 - BitAddr: A0311 - Content: "Hard Limit C-"
ID: 012 - BitAddr: A0312 - Content: "Hard Limit 7th+"
ID: 013 - BitAddr: A0313 - Content: "Hard Limit 7th-"
ID: 014 - BitAddr: A0314 - Content: "Hard Limit 8th+"
ID: 015 - BitAddr: A0315 - Content: "Hard Limit 8th-"
ID: 016 - BitAddr: A0316 - Content: "Main Emegency Switch On"
ID: 017 - BitAddr: A0317 - Content: "Servo Axis 1 Alarm"
ID: 018 - BitAddr: A0318 - Content: "Servo Axis 2 Alarm"
ID: 019 - BitAddr: A0319 - Content: "Servo Axis 3 Alarm"
ID: 020 - BitAddr: A0320 - Content: "Servo Axis 4 Alarm"
ID: 021 - BitAddr: A0321 - Content: "Servo Axis 5 Alarm"
ID: 022 - BitAddr: A0322 - Content: "Servo Axis 6 Alarm"
ID: 023 - BitAddr: A0323 - Content: "Servo Axis 7 Alarm"
ID: 024 - BitAddr: A0324 - Content: "Servo Axis 8 Alarm"
%@WARN_NC_OT(MAX:1000)
ID: 000 - BitAddr: A0350 - Content: "Soft Limit X+"
ID: 001 - BitAddr: A0351 - Content: "Soft Limit X-"
ID: 002 - BitAddr: A0352 - Content: "Soft Limit Y+"
ID: 003 - BitAddr: A0353 - Content: "Soft Limit Y-"
ID: 004 - BitAddr: A0354 - Content: "Soft Limit Z+"
ID: 005 - BitAddr: A0355 - Content: "Soft Limit Z-"
ID: 006 - BitAddr: A0356 - Content: "Soft Limit A+"
ID: 007 - BitAddr: A0357 - Content: "Soft Limit A-"
ID: 008 - BitAddr: A0358 - Content: "Soft Limit B+"
ID: 009 - BitAddr: A0359 - Content: "Soft Limit B-"
ID: 010 - BitAddr: A0360 - Content: "Soft Limit C+"
ID: 011 - BitAddr: A0361 - Content: "Soft Limit C-"
ID: 012 - BitAddr: A0362 - Content: "Soft Limit 7th+"
ID: 013 - BitAddr: A0363 - Content: "Soft Limit 7th-"
ID: 014 - BitAddr: A0364 - Content: "Soft Limit 8th+"
ID: 015 - BitAddr: A0365 - Content: "Soft Limit 8th-"
ID: 016 - BitAddr: A0366 - Content: "Program Soft limit Detected X+"
ID: 017 - BitAddr: A0367 - Content: "Program Soft limit Detected X-"
ID: 018 - BitAddr: A0368 - Content: "Program Soft limit Detected Y+"
ID: 019 - BitAddr: A0369 - Content: "Program Soft limit Detected Y-"
ID: 020 - BitAddr: A0370 - Content: "Program Soft limit Detected Z+"
ID: 021 - BitAddr: A0371 - Content: "Program Soft limit Detected Z-"
ID: 022 - BitAddr: A0372 - Content: "Program Soft limit Detected A+"
ID: 023 - BitAddr: A0373 - Content: "Program Soft limit Detected A-"
ID: 024 - BitAddr: A0374 - Content: "Program Soft limit Detected B+"
ID: 025 - BitAddr: A0375 - Content: "Program Soft limit Detected B-"
ID: 026 - BitAddr: A0376 - Content: "Program Soft limit Detected C+"
ID: 027 - BitAddr: A0377 - Content: "Program Soft limit Detected C-"
ID: 028 - BitAddr: A0378 - Content: "Program Soft limit Detected 7th+"
ID: 029 - BitAddr: A0379 - Content: "Program Soft limit Detected 7th-"
ID: 030 - BitAddr: A0380 - Content: "Program Soft limit Detected 8th+"
ID: 031 - BitAddr: A0381 - Content: "Program Soft limit Detected 8th-"
%@END